Chapter 7. A Distributed 2000 User Network
Prev |  | Next

## Chapter 7. A Distributed 2000 User Network

There is something indeed mystical about things that are big. Large networks exhibit a certain magnetism and exude a sense of importance that obscures reality. You and I know that it is no more difficult to secure a large network than it is a small one. We all know that over and above a particular number of network clients, the rules no longer change; the only real dynamic is the size of the domain (much like a kingdom) over which the network ruler (oops, administrator) has control. The real dynamic then transforms from the technical to the political. Then again, that point is often reached well before the kingdom (or queendom) grows large.

If you have systematically worked your way to this chapter, hopefully you have found some gems and techniques that are applicable in your world. The network designs you have worked with in this book with have their strong points as well as weak ones. That is to be expected given that they are based on real business environments, excepting that the facts have been moulded to serve the purposes of this book.

This chapter is intent on wrapping up issues that are central to implementation and design of progressively larger networks. Are you ready for this chapter? Good, it is time to move on.

In previous chapters, you made the assumption that your network administration staff need detailed instruction right down to the nuts-and-bolts of implementing the solution. That's is still the case, but they have graduated now. You decide to document only those issues, methods and techniques that are new or complex. Routine tasks such as implementing a DNS or a DHCP server are under control. Even the basics of Samba are largely under control. So in this section you focus on the specifics of implementing LDAP changes, Samba changes, and approach and design of the solution and its deployment.

## Introduction

Abmas is a miracle company. Most businesses would have collapsed under the weight of rapid expansion that this company has experienced. Samba is flexible, so there is no need to reinstall the whole operating system just because you need to implement a new network design. In fact, you can keep an old server running right up to the moment of cut-over and then do a near-live conversion. There is no need to reinstall a Samba server just to change the way your network should function.

Network growth is common to all organizations. In this exercise, your preoccupation is with the mechanics of implementing Samba and LDAP so that network users on each network segment can work without impediment.

### Assignment Tasks

Starting with the configuration files for the server called `MASSIVE` in Chapter 6, you now deal with the issues that are particular to large distributed networks. Your task is simple identify the challenges, consider the alternatives, and then design and implement a solution.

Remember, you have users based in London (UK), Los Angeles, Washington DC, and three buildings in New York. A significant portion of your workforce have notebook computers and roam all over the world. Some dial into the office, others use VPN connections over the Internet and others just move between buildings.

What do you say to an employee who normally uses a desktop system but must spend six weeks on the road with a notebook computer? She is concerned over email access and how to keep co-workers current with changing documents.

To top it all off, you have one network support person and one Help desk person based in London, a single person dedicated to all network operations in Los Angeles, five staff for user administration and Help desk in New York, plus one floater for Washington DC.

You have outsourced all desktop deployment and management to DirectPointe,Inc. Your concern is server maintenance and third-level support. Build a plan and show what must be done.

## Dissection and Discussion

In the previous chapter, you implemented an LDAP server that provided the `passdb backend` for the Samba servers. You explored ways to accelerate Windows desktop profile handling and you took control of network performance.

The implementation of an LDAP-based passdb backend (known as ldapsam in Samba parlance), or some form of database that can be distributed, is essential to permit the deployment of Samba Primary and Backup Domain Controllers (PDC/BDCs). You see, the problem is that the tdbsam style passdb backend does not lend itself to being replicated. The older plain-text-based smbpasswd style passdb backend can be replicated using a tool such as rsync, but smbpasswd suffers the drawback that it does not support the range of account facilities demanded by modern network managers.

The new tdbsam facility supports functionality that is similar to an ldapsam, but the lack of distributed infrastructure sorely limits the scope for its deployment. This does raise the following questions: "Why can't I just use an XML based backend, or for that matter, why not use an SQL based backend?" "Is support for these tools broken?" No. Answers to these questions require a bit of background.

What is a directory? A directory is a collection of information regarding objects that can be accessed to rapidly find information that is relevant in a particular and consistent manner. A directory differs from a database in that it is generally more often searched (read) than updated. As a consequence, the information is organized to facilitate read access rather than to support transaction processing.

The Lightweight Directory Access Protocol (LDAP) differs considerably from a traditional database. It has a simple search facility that uniquely makes a highly preferred mechanism for managing user identities. LDAP provides a scalable mechanism for distributing the data repository and for keeping all copies (slaves) in sync with the master repository.

Samba is a flexible and powerful file and print sharing technology. It can use many external authentication sources and can be part of a total authentication and identity management infrastructure. The two most important external sources for large sites are Microsoft Active Directory and LDAP. Sites that specifically wish to avoid the proprietary implications of Microsoft Active Directory naturally gravitate toward OpenLDAP.

In Chapter 6, you had to deal with a locally routed network. All deployment concerns focused around making users happy, and that simply means taking control over all network practices and usage so that no one user is disadvantaged by any other. The real lesson is one of understanding that no matter how much network bandwidth you provide, bandwidth remains a precious resource.

In this chapter, you must now consider how the overall network must function. In particular, you must be concerned with users who move between offices. You must take into account the way users need to access information globally. And you must make the network robust enough so that it can sustain partial breakdown without causing loss of productivity.

### Technical Issues

There are at least three areas that need to be addressed as you approach the challenge of designing a network solution for the newly expanded business. These are:

- User needs such as mobility and data access

- The nature of Windows networking protocols

- Identity management infrastructure needs

Let's look at each in turn.

#### User Needs

The new company has three divisions. Staff for each division are spread across the company. Some staff are office-bound and some are mobile users. Mobile users travel globally. Some spend considerable periods working in other offices. Everyone wants to be able to work without constraint of productivity.

The challenge is not insignificant. In some parts of the world, even dial-up connectivity is poor, while in other regions political encumbrances severely curtail user needs. Parts of the global Internet infrastructure remain shielded-off for reasons outside the scope of this discussion.

Decisions must be made regarding where data is to be stored, how it will be replicated (if at all), and what the network bandwidth implications are. For example, one decision that can be made is to give each office its own master file storage area that can be synchronized to a central repository in New York. This would permit global data to be backed up from a single location. The synchronization tool could be rsync, run via a cron job. Mobile users may use off-line file storage under Windows XP Professional. This way, they can synchronize all files that have changed since each logon to the network.

No matter which way you look at this, the bandwidth requirements for acceptable performance are substantial even if only 10 percent of staff are global data users. A company with 3500 employees and 280 of those were mobile users, and who used a similarly distributed network, found they needed at least 2 Megabit/sec connectivity between the UK and US offices. Even over 2 Mb/s bandwidth, this company abandoned any attempt to run roaming profile usage for mobile users. At that time, the average roaming profile took 480 Kbytes, while today the minimum Windows XP Professional roaming profile involves a transfer of over 750 Kbytes from the profile server to/from the client.

Obviously then, user needs and wide-area practicalities dictate the economic and technical aspects of your network design as well as for standard operating procedures.

#### The Nature of Windows Networking Protocols

Network logons that include roaming profile handling requires from 140 Kbytes to 2 Mbytes. The inclusion of support for a minimal set of common desktop applications can push the size of a complete profile to over 15 Mbytes. This has substantial implications so far as location of user profiles is concerned. Additionally, it is a significant factor in determining the nature and style of mandatory profiles that may be enforced as part of a total service level assurance program that might be implemented.

One way to reduce the network bandwidth impact of user logon traffic is through folder redirection. In Chapter 6, you implemented this in the new Windows XP Professional standard desktop configuration. When desktop folders such as My Documents are redirected to a network drive, they should also be excluded from synchronization to/from the server on logon/out. Redirected folders are analogous to network drive connections.

Of course, network applications should only be run off local application servers. As a general rule, even with 2 Mbit/sec network bandwidth, it would not make sense at all for someone who is working out of the London office to run applications off a server that is located in New York.

When network bandwidth becomes a precious commodity (that is most of the time), there is a significant demand to understand network processes and to mould the limits of acceptability around the constraints of affordability.

When a Windows NT4/200x/XP Professional client user logs onto the network, several important things must happen.

- The client obtains an IP address via DHCP. (DHCP is necessary so that users can roam between offices.)

- The client must register itself with the WINS and/or DNS server.

- The client must locate the closest Domain Controller.

- The client must log onto a Domain Controller and obtain as part of that process the location of the user's profile, load it, connect to redirected folders, and establish all network drive and printer connections.

- The Domain Controller must be able to resolve the user's credentials before the logon process is fully implemented.

Given that this book is about Samba and the fact that it implements the Windows NT4 style domain semantics, it makes little sense to compare Samba with Microsoft Active Directory insofar as the logon protocols and principles of operation are concerned. The following information pertains exclusively to the interaction between a Windows XP Professional workstation and a Samba-3.0.2 server. In the discussion that follows, use is made of DHCP and WINS.

As soon as the Windows workstation starts up, it obtains an IP address. This is immediately followed by registration of its name both by broadcast and Unicast registration that is directed at the WINS server.

Given that the client is already a Domain Member, it then sends a directed (Unicast) request to the WINS server seeking the list of IP addresses for domain controllers (NetBIOS name type 0x1C). The WINS server replies with the information requested.

The client sends two netlogon mailslot broadcast requests to the local network and to each of the IP addresses returned by the WINS server. Whichever answers this request first appears to be the machine that the Windows XP client attempts to use to process the network logon. The mailslot messages use UDP broadcast to the local network and UDP Unicast directed at each machine that was listed in the WINS server response to a request for the list of Domain Controllers.

The logon process begins with negotiation of the SMB/CIFS protocols that are to be used; this is followed by an exchange of information that ultimately includes the client sending the credentials with which the user is attempting to logon. The logon server must now approve the further establishment of the connection, but that is a good point to halt for now. The priority here must center around identification of network infrastructure needs. A secondary fact we need to know is, what happens when local Domain Controllers fail or break?

Under most circumstances, the nearest Domain Controller responds to the netlogon mailslot broadcast. The exception to this norm occurs when the nearest Domain Controller is too busy or is out of service. Herein lies an important fact. This means it is important that every network segment should have at least two Domain Controllers. Since there can be only one Primary Domain Controller (PDC), all additional Domain Controllers are by definition Backup Domain Controllers (BDCs).

The provision of sufficient servers that are BDCs is an important design factor. The second important design factor involves how each of the BDCs obtains user authentication data. That is the subject of the next section as it involves key decisions regarding Identity Management facilities.

#### Identity Management Needs

Network managers recognize that in large organizations users generally need to be given resource access based on needs, while being excluded from other resources for reasons of privacy. It is, therefore, essential that all users identify themselves at the point of network access. The network logon is the principal means by which user credentials are validated and filtered, and appropriate rights and privileges are allocated.

Unfortunately, network resources tend to have their own Identity Management facilities, the quality and manageability of which varies from quite poor to exceptionally good. Corporations that use a mixture of systems soon discover that until recently, few systems were designed to interoperate. For example, UNIX systems each have an independent user database. Sun Microsystems developed a facility that was originally called `Yellow Pages`, and was renamed when a telephone company objected to the use of its trademark. What was once called `Yellow Pages` is today known as `Network Information System` (NIS).

NIS gained a strong following throughout the UNIX/VMS space in a short period of time and retained that appeal and use for over a decade. Security concerns as well as inherent limitations have caused it to enter its twilight. NIS did not gain widespread appeal outside of the UNIX world and was not universally adopted. Sun updated this to a more secure implementation called NIS+, but even it has fallen victim to changing demands as the demand for directory services that can be coupled with other information systems is catching on.

Nevertheless, both NIS and NIS+ continue to hold ground in business areas where UNIX still has major sway. Examples of organizations that remain firmly attached to the use of NIS and NIS+ includes large government departments, education institutions, as well as large corporations that have a scientific or engineering focus.

Today's networking world needs a scalable, distributed Identity Management infrastructure, commonly called a directory. The most popular technologies today are Microsoft Active Directory service and a number of LDAP implementations.

The problem of managing multiple directories has become a focal point over the past decade. This has created a large market for meta-directory products and services that allow organizations that have multiple directories and multiple management and control centers to provision information from one directory into another. The attendant benefit to end users is the promise of having to remember and deal with fewer login identities and passwords.

The challenge of every large network is to find the optimum balance of internal systems and facilities for Identity Management resources. How well the solution is chosen and implemented has potentially significant impact on network bandwidth and systems response needs.

In Chapter 6, you implemented a single LDAP server for the entire network. This may work for smaller networks, but almost certainly fails to meet the needs of large and complex networks. The following section documents how one may implement a single master LDAP server, with multiple slave servers.

What is the best method for implementing master/slave LDAP servers within the context of a distributed 2000 user network is a question that remains to be answered.

One possibility that has great appeal is to create one single large distributed domain. The practical implications of this design (see ???) demands the placement of sufficient BDCs in each location. Additionally, network administrators must make sure that profiles are not transferred over the wide-area links, except as a totally unavoidable measure. Network design must balance the risk of loss of user productivity against the cost of network management and maintenance.

The network design in ??? takes the approach that management of networks that are too remote to be capable of being managed effectively from New York ought to be given a certain degree of autonomy. With this rationale, the Los Angeles and London networks, though fully integrated with that on the east coast of the USA, each have their own domain name space and can be independently managed and controlled. One of the key drawbacks of this design is that it flies in the face of the ability for network users to roam globally without some compromise in how they may access global resources.

Desk-bound users need not be negatively affected by this design, since the use of interdomain trusts can be used to satisfy the need for global data sharing.

When Samba-3 is configured to use an LDAP backend, it stores the domain account information in a directory entry. This account entry contains the domain SID. An unintended but exploitable side effect is that this makes it possible to operate with more than one PDC on a distributed network.

How might this peculiar feature be exploited? The answer is simple. It is imperative that each network segment should have its own WINS server. Major servers on remote network segments can be given a static WINS entry in the `wins.dat` file on each WINS server. This allows all essential data to be visible from all locations. Each location would, however, function as if it is an independent domain, while all sharing the same domain SID. Since all domain account information can be stored in a single LDAP backend, users have unfettered ability to roam.

This concept has not been exhaustively validated, though we can see no reason why this should not work. The important facets are: The name of the domain must be identical in all locations. Each network segment must have its own WINS server. The name of the PDC must be the same in all locations; this necessitates the use of NetBIOS name aliases for each PDC so that they can be accessed globally using the alias and not the PDC's primary name. A single master LDAP server can be based in New York, with multiple LDAP slave servers located on every network segment. Finally, the BDCs should each use fail-over LDAP servers that are in fact slave LDAP servers on the local segments.

With a single master LDAP server, all network updates are effected on a single server. In the event that this should become excessively fragile or network bandwidth limiting, one could implement a delegated LDAP domain. This is also known as a partitioned (or multiple partition) LDAP database and as a distributed LDAP directory.

As the LDAP directory grows, it becomes increasingly important that its structure is implemented in a manner that mirrors organizational needs, so as to limit network update and referential traffic. It should be noted that all directory administrators must of necessity follow the same standard procedures for managing the directory, as retroactive correction of inconsistent directory information can be exceedingly difficult.

Figure 7.1. Network Topology 2000 User Complex Design A

Figure 7.2. Network Topology 2000 User Complex Design B

### Political Issues

As organizations grow, the number of points of control increase also. In a large distributed organization, it is important that the Identity Management system must be capable of being updated from many locations, and it is equally important that changes made should become capable of being used in a reasonable period, typically minutes rather than days (the old limitation of highly manual systems).

## Implementation

Samba-3 has the ability to use multiple password (authentication and identity resolution) backends. The diagram in ??? demonstrates how Samba uses winbind, LDAP, and NIS, the traditional system password database. The diagram only documents the mechanisms for authentication and identity resolution (obtaining a UNIX UID/GID) using the specific systems shown.

Figure 7.3. Samba and Authentication Backend Search Pathways

Samba is capable of using the `smbpasswd`, `tdbsam`, `xmlsam`, and `mysqlsam` authentication databases. The SMB passwords can, of course, also be stored in an LDAP ldapsam backend. LDAP is the preferred passdb backend for distributed network operations.

Additionally, it is possible to use multiple passdb backends concurrently as well as have multiple LDAP backends. As a result, one can specify a fail-over LDAP backend. The syntax for specifying a single LDAP backend in `smb.conf` is:

    ...
    passdb backend = ldapsam:ldap://master.abmas.biz
    ...

This configuration tells Samba to use a single LDAP server as shown in ???.

Figure 7.4. Samba Configuration to Use a Single LDAP Server

The addition of a fail-over LDAP server can simply be done by adding a second entry for the fail-over server to the single `ldapsam` entry as shown here (note the particular use of the double quotes):

    ...
    passdb backend = ldapsam:"ldap://master.abmas.biz \
    	                  ldap://slave.abmas.biz"
    ...

This configuration tells Samba to use a master LDAP server, with fail-over to a slave server if necessary, as shown in ???.

Figure 7.5. Samba Configuration to Use a Dual (Fail-over) LDAP Server

Some folks have tried to implement this without the use of double quotes as shown above. This is the type of entry they had created:

    ...
    passdb backend = ldapsam:ldap://master.abmas.biz \
                     ldapsam:ldap://slave.abmas.biz
    ...

The effect of this style of entry is that Samba lists the users that are in both LDAP databases. If both contain the same information, it results in each record being shown twice. This is, of course, not the solution desired for a fail-over implementation. The net effect of this configuration is shown in ???

Figure 7.6. Samba Configuration to Use Dual LDAP Databases - Broken - Do Not Use!

If, however, each LDAP database contains unique information, this may well be an advantageous way to effectively integrate multiple LDAP databases into one seemingly contiguous directory. Only the first database will be updated. An example of this configuration is shown in ???.

Figure 7.7. Samba Configuration to Use Two LDAP Databases - The result is additive.

### Note

When the use of ldapsam is specified twice, as shown here, it is imperative that the two LDAP directories must be disjoint. If the entries are for a master LDAP server as well as its own slave server, updates to the LDAP database may end up being lost or corrupted. You may safely use multiple LDAP backends only so long as both are entirely separate from each other.

It is assumed that the network you are working with follows in a pattern similar to what has been covered in Chapter 6. The following steps permit the operation of a Master/Slave OpenLDAP arrangement.

1. Log onto the master LDAP server as `root`. You are about to change the configuration of the LDAP server, so it makes sense to temporarily halt it. Stop OpenLDAP from running on SUSE Linux by executing:

       root#  rcldap stop

   On Red Hat Linux, you can do this by executing:

       root#  service ldap stop

2. Edit the `/etc/openldap/slapd.conf` file so it matches the content of ???.

3. Create a file called `admin-accts.ldif` with the following contents:

       dn: cn=updateuser,dc=abmas,dc=biz
       objectClass: person
       cn: updateuser
       sn: updateuser
       userpaddword: not24get

       dn: cn=sambaadmin,dc=abmas,dc=biz
       objectClass: person
       cn: sambaadmin
       sn: sambaadmin
       userpaddword: buttercup

4. Add an account called “updateuser” to the master LDAP server as shown here:

       root#  slapadd -v -l admin-accts.ldif

5. Change directory to a suitable place to dump the contents of the LDAP server. The dump file (and LDIF file) is used to preload the Slave LDAP server database. You can dump the database by executing:

       root#  slapcat -v -l LDAP-transfer-LDIF.txt

   Each record is written to the file.

6. Copy the file `LDAP-transfer-LDIF.txt` to the intended slave LDAP server. A good location could be in the directory `/etc/openldap/preload`.

7. Log onto the slave LDAP server as `root`. You can now configure this server so the `/etc/openldap/slapd.conf` file matches the content of ???.

8. Change directory to the location in which you stored the `LDAP-transfer-LDIF.txt` file (`/etc/openldap/preload`). While in this directory, execute:

       root#  slapadd -v -l LDAP-transfer-LDIF.txt

   If all goes well, the following output confirms that the data is being loaded as intended:

       added: "dc=abmas,dc=biz" (00000001)
       added: "cn=sambaadmin,dc=abmas,dc=biz" (00000002)
       added: "cn=updateuser,dc=abmas,dc=biz" (00000003)
       added: "ou=People,dc=abmas,dc=biz" (00000004)
       added: "ou=Groups,dc=abmas,dc=biz" (00000005)
       added: "ou=Computers,dc=abmas,dc=biz" (00000006)
       added: "uid=Administrator,ou=People,dc=abmas,dc=biz" (00000007)
       added: "uid=nobody,ou=People,dc=abmas,dc=biz" (00000008)
       added: "cn=Domain Admins,ou=Groups,dc=abmas,dc=biz" (00000009)
       added: "cn=Domain Users,ou=Groups,dc=abmas,dc=biz" (0000000a)
       added: "cn=Domain Guests,ou=Groups,dc=abmas,dc=biz" (0000000b)
       added: "uid=bobj,ou=People,dc=abmas,dc=biz" (0000000c)
       added: "sambaDomainName=MEGANET2,dc=abmas,dc=biz" (0000000d)
       added: "uid=stans,ou=People,dc=abmas,dc=biz" (0000000e)
       added: "uid=chrisr,ou=People,dc=abmas,dc=biz" (0000000f)
       added: "uid=maryv,ou=People,dc=abmas,dc=biz" (00000010)
       added: "cn=Accounts,ou=Groups,dc=abmas,dc=biz" (00000011)
       added: "cn=Finances,ou=Groups,dc=abmas,dc=biz" (00000012)
       added: "cn=PIOps,ou=Groups,dc=abmas,dc=biz" (00000013)

9. Now start the LDAP server and set it to run automatically on system reboot by executing:

       root#  rcldap start
       root#  chkconfig ldap on

   On Red Hat Linux, you would execute the following:

       root#  service ldap start
       root#  chkconfig ldap on

10. Go back to the master LDAP server. Execute the following to start LDAP as well as slurpd, the synchronization daemon, as shown here:

        root#  rcldap start
        root#  chkconfig ldap on
        root#  rcslurpd start
        root#  chkconfig slurpd on

    On Red Hat Linux, check the equivalent command to start slurpd.

11. On the master ldap server you may now add an account to validate that replication is working. Assuming the configuration shown in Chapter 6, execute:

        root#  /var/lib/samba/sbin/smbldap-useradd.pl -a fruitloop

12. On the slave LDAP server, change to the directory `/var/lib/ldap`. There should now be a file called `replogfile`. If replication worked as expected, the content of this file should be:

        time: 1072486403
        dn: uid=fruitloop,ou=People,dc=abmas,dc=biz
        changetype: modify
        replace: sambaProfilePath
        sambaProfilePath: \\MASSIVE\profiles\fruitloop
        -
        replace: sambaHomePath
        sambaHomePath: \\MASSIVE\homes
        -
        replace: entryCSN
        entryCSN: 2003122700:43:38Z#0x0005#0#0000
        -
        replace: modifiersName
        modifiersName: cn=Manager,dc=abmas,dc=biz
        -
        replace: modifyTimestamp
        modifyTimestamp: 20031227004338Z
        -

13. Given that this first slave LDAP server is now working correctly, you may now implement additional slave LDAP servers as required.

Example 7.1. LDAP Master Server Configuration File `/etc/openldap/slapd.conf`

    include     /etc/openldap/schema/core.schema
    include     /etc/openldap/schema/cosine.schema
    include     /etc/openldap/schema/inetorgperson.schema
    include     /etc/openldap/schema/nis.schema
    include     /etc/openldap/schema/samba.schema

    pidfile     /var/run/slapd/slapd.pid
    argsfile    /var/run/slapd/slapd.args

    database    ldbm
    suffix      "dc=abmas,dc=biz"
    rootdn      "cn=Manager,dc=abmas,dc=biz"

    # rootpw = not24get
    rootpw      {SSHA}86kTavd9Dw3FAz6qzWTrCOKX/c0Qe+UV

    replica     host=lapdc.abmas.biz:389
                suffix="dc=abmas,dc=biz"
                binddn="cn=updateuser,dc=abmas,dc=biz"
                bindmethod=simple credentials=not24get

    access to attrs=sambaLMPassword,sambaNTPassword
               by dn="cn=updateuser,dc=abmas,dc=biz" write
               by * none

    replogfile  /var/lib/ldap/replogfile

    directory   /var/lib/ldap

    # Indices to maintain
    index objectClass           eq
    index cn                    pres,sub,eq
    index sn                    pres,sub,eq
    index uid                   pres,sub,eq
    index displayName           pres,sub,eq
    index uidNumber             eq
    index gidNumber             eq
    index memberUID             eq
    index sambaSID              eq
    index sambaPrimaryGroupSID  eq
    index sambaDomainName       eq
    index default               sub

Example 7.2. LDAP Slave Configuration File `/etc/openldap/slapd.conf`

    include     /etc/openldap/schema/core.schema
    include     /etc/openldap/schema/cosine.schema
    include     /etc/openldap/schema/inetorgperson.schema
    include     /etc/openldap/schema/nis.schema
    include     /etc/openldap/schema/samba.schema

    pidfile     /var/run/slapd/slapd.pid
    argsfile    /var/run/slapd/slapd.args

    database    ldbm
    suffix      "dc=abmas,dc=biz"
    rootdn      "cn=Manager,dc=abmas,dc=biz"

    # rootpw = not24get
    rootpw      {SSHA}86kTavd9Dw3FAz6qzWTrCOKX/c0Qe+UV

    access to *
                by dn=cn=updateuser,dc=abmas,dc=biz write
                by * read

    updatedn    cn=updateuser,dc=abmas,dc=biz
    updateref   ldap://massive.abmas.biz

    directory   /var/lib/ldap

    # Indices to maintain
    index objectClass           eq
    index cn                    pres,sub,eq
    index sn                    pres,sub,eq
    index uid                   pres,sub,eq
    index displayName           pres,sub,eq
    index uidNumber             eq
    index gidNumber             eq
    index memberUID             eq
    index sambaSID              eq
    index sambaPrimaryGroupSID  eq
    index sambaDomainName       eq
    index default               sub

Example 7.3. Primary Domain Controller smb.conf File Part A

# Global parameters
`[global]`
`unix charset = LOCALE`
`workgroup = MEGANET2`
`passdb backend = ldapsam:ldap://massive.abmas.biz`
`username map = /etc/samba/smbusers`
`log level = 1`
`syslog = 0`
`log file = /var/log/samba/%m`
`max log size = 0`
`smb ports = 139 445`
`name resolve order = wins bcast hosts`
`time server = Yes`
`printcap name = CUPS`
`add user script = /var/lib/samba/sbin/smbldap-useradd.pl -m '%u'`
`delete user script = /var/lib/samba/sbin/smbldap-userdel.pl '%u'`
`add group script = /var/lib/samba/sbin/smbldap-groupadd.pl -p '%g'`
`delete group script = /var/lib/samba/sbin/smbldap-groupdel.pl '%g'`
`add user to group script = /var/lib/samba/sbin/`
`smbldap-groupmod.pl -m '%g' '%u'`
`delete user from group script = /var/lib/samba/sbin/`
`smbldap-groupmod.pl -x '%g' '%u'`
`set primary group script = /var/lib/samba/sbin/`
`smbldap-usermod.pl -g '%g' '%u'`
`add machine script = /var/lib/samba/sbin/`
`smbldap-useradd.pl -w '%u'`
`shutdown script = /var/lib/samba/scripts/shutdown.sh`
`abort shutdown script = /sbin/shutdown -c`
`logon script = scripts\logon.bat`
`logon path = \\%L\profiles\%U`
`logon drive = X:`
`domain logons = Yes`
`domain master = Yes`
`wins support = Yes`
`ldap suffix = dc=abmas,dc=biz`
`ldap machine suffix = ou=People`
`ldap user suffix = ou=People`
`ldap group suffix = ou=Groups`
`ldap idmap suffix = ou=Idmap`
`ldap admin dn = cn=Manager,dc=abmas,dc=biz`
`idmap backend = ldap://massive.abmas.biz`
`idmap uid = 10000-20000`
`idmap gid = 10000-20000`
`printer admin = root`
`printing = cups`

Example 7.4. Primary Domain Controller smb.conf File Part B

`[IPC$]`
`path = /tmp`
`[accounts]`
`comment = Accounting Files`
`path = /data/accounts`
`read only = No`
`[service]`
`comment = Financial Services Files`
`path = /data/service`
`read only = No`
`[pidata]`
`comment = Property Insurance Files`
`path = /data/pidata`
`read only = No`
`[homes]`
`comment = Home Directories`
`valid users = %S`
`read only = No`
`browseable = No`
`[printers]`
`comment = SMB Print Spool`
`path = /var/spool/samba`
`guest ok = Yes`
`printable = Yes`
`browseable = No`

Example 7.5. Primary Domain Controller smb.conf File Part C

`[apps]`
`comment = Application Files`
`path = /apps`
`admin users = bjones`
`read only = No`
`[netlogon]`
`comment = Network Logon Service`
`path = /var/lib/samba/netlogon`
`admin users = root, Administrator`
`guest ok = Yes`
`locking = No`
`[profiles]`
`comment = Profile Share`
`path = /var/lib/samba/profiles`
`read only = No`
`profile acls = Yes`
`[profdata]`
`comment = Profile Data Share`
`path = /var/lib/samba/profdata`
`read only = No`
`profile acls = Yes`
`[print$]`
`comment = Printer Drivers`
`path = /var/lib/samba/drivers`
`write list = root`
`admin users = root, Administrator`

Example 7.6. Backup Domain Controller smb.conf File Part A

# # Global parameters
`[global]`
`unix charset = LOCALE`
`workgroup = MEGANET2`
`netbios name = BLDG1`
`passdb backend = ldapsam:ldap://lapdc.abmas.biz`
`username map = /etc/samba/smbusers`
`log level = 1`
`syslog = 0`
`log file = /var/log/samba/%m`
`max log size = 50`
`smb ports = 139 445`
`name resolve order = wins bcast hosts`
`printcap name = CUPS`
`show add printer wizard = No`
`logon script = scripts\logon.bat`
`logon path = \\%L\profiles\%U`
`logon drive = X:`
`domain logons = Yes`
`os level = 63`
`domain master = No`
`wins server = 192.168.2.1`
`ldap suffix = dc=abmas,dc=biz`
`ldap machine suffix = ou=People`
`ldap user suffix = ou=People`
`ldap group suffix = ou=Groups`
`ldap idmap suffix = ou=Idmap`
`ldap admin dn = cn=Manager,dc=abmas,dc=biz`
`utmp = Yes`
`idmap backend = ldap://massive.abmas.biz`
`idmap uid = 10000-20000`
`idmap gid = 10000-20000`
`printing = cups`
`[accounts]`
`comment = Accounting Files`
`path = /data/accounts`
`read only = No`
`[service]`
`comment = Financial Services Files`
`path = /data/service`
`read only = No`

Example 7.7. Backup Domain Controller smb.conf File Part B

`[pidata]`
`comment = Property Insurance Files`
`path = /data/pidata`
`read only = No`
`[homes]`
`comment = Home Directories`
`valid users = %S`
`read only = No`
`browseable = No`
`[printers]`
`comment = SMB Print Spool`
`path = /var/spool/samba`
`guest ok = Yes`
`printable = Yes`
`browseable = No`
`[apps]`
`comment = Application Files`
`path = /apps`
`admin users = bjones`
`read only = No`
`[netlogon]`
`comment = Network Logon Service`
`path = /var/lib/samba/netlogon`
`guest ok = Yes`
`locking = No`
`[profiles]`
`comment = Profile Share`
`path = /var/lib/samba/profiles`
`read only = No`
`profile acls = Yes`
`[profdata]`
`comment = Profile Data Share`
`path = /var/lib/samba/profdata`
`read only = No`
`profile acls = Yes`

### Key Points Learned

- Where Samba-3 is used as a Domain Controller, the use of LDAP is an essential component necessary to permit the use of BDCs.

- Replication of the LDAP master server to create a network of BDCs is an important mechanism for limiting wide-area network traffic.

- Network administration presents many complex challenges, most of which can be satisfied by good design, but that also require sound communication and unification of management practices. This can be highly challenging in a large, globally distributed network.

- Roaming profiles must be contained to the local network segment. Any departure from this may clog wide-area arteries and slow legitimate network traffic to a crawl.

## Questions and Answers

There is much rumor and misinformation regarding the use of MS Windows networking protocols. These questions are just a few of those frequently asked.

DHCPnetworkbandwidth Is it true that DHCP uses lots of wide-area network bandwidth?
background communicationLDAPmaster/slavebackground communication How much background communication takes place between a Master LDAP server and its slave LDAP servers?
LDAP has a database. Is LDAP not just a fancy database front end?
OpenLDAP Can Active Directory obtain account information from an OpenLDAP server?
What are the parts of a roaming profile? How large is each part?
Can the My Documents folder be stored on a network drive?
wide-areanetworkbandwidthWINS How much wide-area network bandwidth does WINS consume?
How many BDCs should I have? What is the right number of Windows clients per server?
NIS serverLDAP I've heard that you can store NIS accounts in LDAP. Is LDAP not just a smarter way to run an NIS server?
Can I use NIS in place of LDAP?

| Is it true that DHCP uses lots of wide-area network bandwidth?
| It is a smart practice to localize DHCP servers on each network segment. As a rule, there should be two DHCP servers per network segment. This means that if one server fails, there is always another to service user needs. DHCP requests use only UDP broadcast protocols. It is possible to run a DHCP Relay Agent on network routers. This makes it possible to run fewer DHCP servers. A DHCP network address request and confirmation usually results in about six UDP packets. The packets are from 60 to 568 bytes in length. Let us consider a site that has 300 DHCP clients and that uses a 24-hour IP address lease. This means that all clients renew their IP address lease every 24 hours. If we assume an average packet length equal to the maximum (just to be on the safe side), and we have a 128 Kbit/sec wide-area connection, how significant would the DHCP traffic be if all of it were to use DHCP Relay? I must stress that this is a bad design, but here is the calculation:
    Daily Network Capacity: 128,000 (Kbits/s) / 8 (bits/byte)
                                 x 3600 (sec/hr) x 24 (hrs/day)= 2288 Mbytes/day.

    DHCP traffic:          300 (clients) x 6 (packets)
                                           x 512 (bytes/packet) = 0.9 Mbytes/day.
From this can be seen that the traffic impact would be minimal. Even when DHCP is configured to do DNS update (Dynamic DNS) over a wide-area link, the impact of the update is no more than the DHCP IP address renewal traffic and, thus, still insignificant for most practical purposes.
| How much background communication takes place between a Master LDAP server and its slave LDAP servers?
| The process that controls the replication of data from the Master LDAP server to the Slave LDAP servers is called slurpd. The slurpd remains nascent (quiet) until an update must be propagated. The propagation traffic per LDAP salve to update (add/modify/delete) two user accounts requires less than 10Kbytes traffic.
| LDAP has a database. Is LDAP not just a fancy database front end?
| LDAP does store its data in a database of sorts. In fact the LDAP backend is an application-specific data storage system. This type of database is indexed so that records can be rapidly located, but the database is not generic and can be used only in particular pre-programmed ways. General external applications do not gain access to the data. This type of database is used also by SQL servers. Both an SQL server and an LDAP server provide ways to access the data. An SQL server has a transactional orientation and typically allows external programs to perform ad-hoc queries, even across data tables. An LDAP front end is a purpose-built tool that has a search orientation that is designed around specific simple queries. The term `database` is heavily overloaded and, thus, much misunderstood.
| Can Active Directory obtain account information from an OpenLDAP server?
| No, at least not directly. It is possible to provision Active Directory from/to an OpenLDAP database through use of a meta-directory server. Microsoft MMS (now called MIIS) can interface to OpenLDAP using standard LDAP queries/updates.
| What are the parts of a roaming profile? How large is each part?
| A roaming profile consists of: Desktop folders such as: `Desktop, My Documents, My Pictures, My Music, Internet Files, Cookies, Application Data, Local Settings,` and more. See ???. Each of these can be anywhere from a few bytes to gigabytes in capacity. Fortunately, all such folders can be redirected to network drive resources. See ??? for more information regarding folder redirection. A static or re-writable portion that is typically only a few files (2-5 Kbytes of information). The registry load file that modifies the `HKEY_LOCAL_USER` hive. This is the `NTUSER.DAT` file. It can be from 0.4-1.5 MBytes. Microsoft Outlook PST files may be stored in the `Local Settings\Application Data` folder. It can be up to 2 Gbytes in size per PST file.
| Can the `My Documents` folder be stored on a network drive?
| Yes. More correctly, such folders can be redirected to network shares. No specific network drive connection is required. Registry settings permit this to be redirected directly to a UNC (Universal Naming Convention) resource, though it is possible to specify a network drive letter instead of a UNC name. See ???.
| How much wide-area network bandwidth does WINS consume?
| MS Windows clients cache information obtained from WINS lookups in a local NetBIOS name cache. This keeps WINS lookups to a minimum. On a network with 3500 MS Windows clients and a central WINS server, the total bandwidth demand measured at the WINS server, averaged over an eight-hour working day, was less than 30 Kbytes/sec. Analysis of network traffic over a six-week period showed that the total of all background traffic consumed about 11 percent of available bandwidth over 64 Kbit/sec links. Back-ground traffic consisted of domain replication, WINS queries, DNS lookups, authentication traffic. Each of 11 branch offices had a 64 Kbit/sec wide-area link, with a 1.5 Mbit/sec main connection that aggregated the branch office connections plus an Internet connection. In conclusion, the total load afforded through WINS traffic is again marginal to total operational usage as it should be.
| How many BDCs should I have? What is the right number of Windows clients per server?
| It is recommended to have at least one BDC per network segment, including the segment served by the PDC. Actual requirements vary depending on the working load on each of the BDCs and the load demand pattern of client usage. I have seen sites that function without problem with 200 clients served by one BDC, and yet other sites that had one BDC per 20 clients. In one particular company, there was a drafting office that has 30 CAD/CAM operators served by one server, a print server; and an application server. While all three were BDCs, typically only the print server would service network logon requests after the first 10 users had started to use the network. This was a reflection of the service load placed on both the application server and the data server. As unsatisfactory as the answer might sound, it all depends on network and server load characteristics.
| I've heard that you can store NIS accounts in LDAP. Is LDAP not just a smarter way to run an NIS server?
| The correct answer to both questions is yes. But do understand that an LDAP server has a configurable schema that can store far more information for many more purposes than just NIS.
| Can I use NIS in place of LDAP?
| No. The NIS database does not have provision to store Microsoft encrypted passwords and does not deal with the types of data necessary for interoperability with Microsoft Windows networking. The use of LDAP with Samba requires the use of a number of schemas, one of which is the NIS schema, but also a Samba-specific schema extension.

Prev | Up | Next
Chapter 6. Making Users Happy | Home | Chapter 8. Migrating NT4 Domain to Samba-3