# Editing a SANbox2 or SANbox2-64 Zone Set

You can NOT edit an active zone set using a SANbox2 or SANbox2-64 switch. You must configure a deactivated zone set to your needs and then activate that updated zone set to apply the changes to the fabric.

To edit a zone set on a SANbox2 or SANbox2-64 switch and apply those changes to the fabric, do the following:

1. In the faceplate display, open the Zoning menu and select Edit Zoning.

2. In the Edit Zoning dialog, select a deactivated zone set in the zone set tree.

3. Configure the deactivated zone set to your needs.

4. Click the OK button to save the zoning changes.

5. In the faceplate display, open the Zoning menu and select Activate Zone Set.

6. In the Activate Zoneset dialog, select the newly configured zone set from the pull-down menu.

7. Click the Activate button.

Important! To apply zoning changes you made to a fabric using a SANbox2 or SANbox2-64 switch, you must activate the updated zone set.