# Changing the Pending Firmware

To change the pending firmware to the alternate image, do the following:

1. In the faceplate display, open the Switch menu and select Firmware Fallback.

2. The Firmware Fallback dialog prompts you to confirm the firmware version that is to become the pending firmware. Click the Yes button to select the fallback firmware or click the No button to cancel.

3. SANbox Manager attempts a non-disruptive activation if the current and pending firmware version is 2.0 or greater. Otherwise, SANbox Manager prompts you reset the switch to activate the pending firmware.