# SANbox Edit Zoning Dialog

The Edit Zoning dialog has a zone set tree on the left and a port/device tree (or members) on the right. Both trees expand and contract zone sets, zones, and ports. An expanded port shows the port Fibre Channel address; and expanded address shows the port worldwide name. Zoned devices no longer present in the fabric are grayed-out.

To edit the zoning database for a particular switch, open the faceplate display, open the Switch menu, and select Zoning. Using menu options, buttons, popup menus, and/or drag-and-drop, you can create and manage zone sets and zones, and save the changes to the zoning database.

Edit Zoning Buttons

Create Zone Set button | Creates a new zone set
Create Zone button | Creates a new zone
Create Alias button | Not applicable
Add Member button | Adds the selected zone to a zone set, or adds the selected port to a zone
Remove Member button | Deletes the selected zone from a zone set or, deletes the selected port from a zone