# Configuring Traps

The trap log (on SANbox with E_Ports only) displays the system event information related to user-configured conditions.

To configure a trap on a SANbox switch, do the following:

1. Open the SANbox faceplate display, and select Configure Traps to open the Trap Configuration dialog.

2. Check the Enable All Traps box to activate all configured traps.

3. Enter a value in the Sample Interval field.

4. In the Trap pull-down menu, select a trap type.

5. Enter values in the Rising Threshold and Falling Threshold fields.

6. Check the Enable box to enable this trap, or remove the check mark to disable this trap.

7. Click the OK button to save the changes.