# Replacing a Failed Switch in a Fabric

To replace a failed switch in a fabric, plug in the switch and copy the archived switch configuration file to the switch using the Restore function.

Note: The switch configuration must be archived before it can be restored.

To replace a failed switch using the SANbox Manager Restore function, do the following:

1. Unplug and remove the failed switch.

2. Plug in the new replacement switch.

3. Open the topology display and select the replacement switch.

4. Open the Switch menu and select Restore.

5. In the Restore Switch dialog, enter a name or choose the archived switch configuration file to copy to the switch.

6. Click the OK button to write the configuration file to the switch.