# SANbox2 Switch Factory Configuration Settings

The default out-of-the-box factory settings for a SANbox2 switch are listed below. Note: Restoring the switch to the factory default configuration does not restore the login name and password settings. You must use the Reset Password File button in the Maintenance Mode screen.

Symbolic Name | SANbox2
Administrative State | Online
Domain ID | 1 (0x Hex)
Domain ID Lock | False
Resource Allocation Timeout (RA TOV) | 10000 milliseconds
Error Detect Timeout (ED TOV) | 2000 milliseconds
IP Address | 10.0.0.1
Subnet Mask Address | 255.0.0.0
Gateway Address | 10.0.0.254
Network Discovery | RARP
Enable Remote Logging | Disabled
Logging Host IP Address | 10.0.0.254
Inband Enabled | True
Broadcast Enabled | True
I/O Stream Guard | Disabled
Configuration Description | SANbox2 FC Switch
Trap 1 Address | 10.0.0.254
Trap [2-5] Addresses | 0.0.0.0
Trap [1-5] Port | 162
Trap [1-5] Severity | Warning
Trap [1-5] Enabled | Disabled
Threshold Monitoring Enabled | Disabled
CRC Errors Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 25 1 10
Decode Errors Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 200 0 10
ISL Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 2 0 10
Login Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 5 1 10
Logout Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 5 1 10
LOS Monitoring Enabled * Rising Trigger * Falling Trigger * Sample Window | True 100 5 10
Contact | <syscontact>
Location | <sysLocation>
Trap Community | Public
Read Community | Public
Write Community | Private
Port State | Online
Port Speed | Auto-detect
Port Mode | GL