# Installing Firmware on a Switch

Installing firmware involves loading, unpacking, and activating the firmware image on the switch. SANbox Manager does this in one operation.

Note: For firmware versions that follow the initial release of version 2.0, you have the ability to install and activate new firmware without resetting the switch, and therefore, without disrupting traffic. SANbox Manager will attempt a non-disruptive firmware installation and activation whenever possible.

To install firmware on a switch, do the following:

1. In the faceplate display, open the Switch menu and select Load Firmware.

2. In the Firmware Upload dialog, click the Select button to browse and select the firmware file to be uploaded.

3. Click the Start button to begin the firmware load process.

4. When the loading is complete, click the Close button to close the Firmware Upload dialog.

5. If a non-disruptive installation is not possible, SANbox Manager prompts you to reset the switch. Click the OK button to reset the switch and activate the new firmware.