# Topology Display Data Windows

The topology display data window tabs for SANbox with E_Ports, SANbox2, and SANbox2-64 switches are Name Server, Active Zoneset, Switch, and Link. Click a data window tab to display its content in the data window above.

Name Server Data Window

Displays all devices connected to the switch that are logged with the name server.

Target/Initiator | Device type: target or initiator
Switch | Switch name
Port | Port number (0 - 15)
Address | Fibre Channel address
Type | Node type
Node WWN | Node worldwide name
Port WWN | Port worldwide name
Vendor | Host bus adapter vendor
FC-4 Types | Device Fibre Channel protocol types
Active Zones | Displays the zones (if any) in which Name Server entry is a member.

Active Zoneset Data Window

The Active Zoneset data window is a graphical representation of the zone membership for the active zone set. To open the Active Zoneset data window, choose the Active Zoneset tab below the data window in the topology display. The active zone set shown in this window is a compilation of zone sets with the same name from all switches in the fabric.

Switch Data Window

Displays current network and switch configuration data.

FcAddress | Switch Fibre Channel address
World Wide Name | Switch worldwide name
Reason for Status | Additional status information
User Name | Name of user
Login Level | Security level
Security Enabled | User Authentication Security (True/False). If true, the user must enter a valid account name/password combination before gaining access to a switch.
Vendor | Switch manufacturer
Flash Version | Active firmware version
Inactive Flash Version | Inactive firmware version
Pending Flash Version | Firmware version that will be activated at the next reset
PROM/Flasher Version | PROM firmware version
MAC Address | Media Access Control address
IP Address | Internet Protocol Address
Subnet Mask | Mask that determines the IP address subnet
Gateway | Gateway address
Negotiated Domain ID | The domain ID currently being used by the fabric
Configured Domain ID | The domain ID defined by network administrator
Domain ID Lock | Domain ID lock status. Prevents (True) or permits (False) dynamic domain ID reassignment.
Number of Ports | Number of ports on the switch
Switch Type | Switch model
Operational State | Switch operational state: Online, Offline, Diagnostic
Administrative State | Switch administrative state: Online, Offline, Diagnostic
MFS Timeout | Multi-frame sequencing timeout value
RA Timeout | Resource allocation timeout value
ED Timeout | Error detect timeout value
FC-SW-2 Auto Save | Zoning auto save status. Saves zoning updates in temporary and permanent memory (True) or only in temporary memory (False).
FC-SW-2 Compliant | Zoning merge status. If True, changes to the active zone set are propagated throughout the fabric. If False, changes to the zoning database are propagated throughout the fabric.
Zoning Default Visibility | Zoning visibility status. Permits (All) or prevents (None) communication with other switches in the absence of an active zone set.
Legacy Address Format | Legacy port addressing status. Enabled only for interoperability with non-FC-SW-2 switches.
Temperature | Internal switch temperature (in Celsius)
Fan 1 Status | Fan 1 Status
Fan 2 Status | Fan 2 Status
Fan 3 Status | Fan 3 Status
Power Supply 1 Status | Power Supply 1 Status
Power Supply 2 Status | Power Supply 2 Status
Beacon Status | Whether LEDs on switch are blinking
Broadcast Support | Whether broadcast support is enabled or disabled
Inband Enabled | Inband management status. Permits (True) or prevents (False) a switch from being managed over an ISL.
Temperature Failure Port Shutdown | Port shutdown status. If True, all ports are downed when the switch temperature exceeds the Failure Temperature. If False, port operational states remain unchanged.
Warning Temperature | Warning temperature threshold in °C above which a warning condition alarm is generated.
Failure Temperature | Failure temperature threshold in °C above which a failure condition alarm is generated.

Link Data Window

Status | Current link status
Switch 1 | The first switch discovered in the fabric.
Switch 2 | The second switch discovered in the fabric.