# Starting SANbox Manager on Solaris

To start the SANbox Manager application for the first time, do the following:

1. Enter the following SANbox Manager command:

/usr/opt/SUNWsmgr2/bin/SANbox_Manager

2. The very first time you start the SANbox Manager application or if the default fabric view file does not exist, a blank topology window is displayed in which to add a fabric. Open the Fabric menu and select Add Fabric, or choose the Add button in the tool bar to open the Add a New Fabric dialog.

Note: If the default fabric view file was saved with a password in a previous session, SANbox Manager will automatically open the default fabric file after you enter the password in the Load Default File Password dialog and click the Load View File button. To not open the saved default fabric view file and open the Add a New Fabric dialog, click the Continue Without Loading button in the Load Default File Password dialog.

3. In the Fabric Name field, enter a name for the fabric.

4. In the IP address field, enter the IP address of the fabric.

5. In the Login Name field, enter your login name.

6. In the Password field, enter the password (the default is "password"). If security is turned off (default), you are not required to enter a login name or password.

7. Click the Add Fabric button.

Note: A switch supports a combined maximum of 19 logins reserved as follows:

* 4 sessions for internal applications such as management server and SNMP

* 15 sessions for SANbox Manager inband and out-of-band logins, Application Programming Interface (API) inband and out-of-band logins, and Telnet logins. Of these 15, there can be a combined maximum of 10 SANbox Manager and API logins. Additional logins will be refused.