# SANbox2 Edit Zoning Dialog

The Edit Zoning dialog has a zone set tree on the left side, and a port/device (or members) tree on the right side. Both trees expand and contract zone sets, zones, and ports. An expanded port shows the port Fibre Channel address; and expanded address shows the port worldwide name. Zoned devices no longer present in the fabric are grayed-out.

To edit the zoning database for a particular switch, open the faceplate display, open the Switch menu, and select Zoning to display the Edit Zoning dialog. Using menu options, buttons, popup menus, and/or drag-and-drop, you can create and manage zone sets and zones, and save the changes to the zoning database.

Before requested zoning changes are applied, SANbox Manager checks for possible zoning violations and informs the user of possible zoning conflicts (listed below).

* Empty zone sets

* Empty zones

* Empty alias

* ACL or VPF zone with non-domain port members

* Members in VPF zones that are in another VPF zone.

* Members in the same ACL zone that are segmented by VPF zoning.

* Members in the same soft zone that are segmented by VPF or ACL zoning.

To select zone sets, zones, or ports:

* Click a zone, zone set, or port icon.

* Hold down the Shift key while clicking several consecutive icons.

* Hold down the Control key while clicking several non-consecutive icons.

* Right-click a zone or a zone set, and its corresponding popup menu will open.

Edit Zoning Buttons

Create Zone Set button | Creates a new zone set
Create Zone button | Creates a new zone
Create Alias button | Creates another name for a set of objects
Add Member button | Adds the selected zone to a zone set, or adds the selected port to a zone
Remove Member button | Deletes the selected zone from a zone set or, deletes the selected port from a zone