# Refreshing Switch Information

The Refresh Switch option starts a new polling cycle to update the currently displayed fabric information. The polling frequency (in Preferences) defines how often SANbox Manager polls the fabric to obtain the current fabric status and display it in the topology display or faceplate display.

To immediately refresh the status in the display, do one of the following:

* Click the Refresh button.

* Open the View menu and select Refresh.

* Press the F5 key.

* Right-click a switch in the topology display and select Refresh Switch from the popup menu.

* Right-click in the graphic window of the faceplate display, and select Refresh Switch from the popup menu.