# SANbox Switch Factory Configuration Settings

The default out-of-the-box factory settings for a SANbox with E_Ports switch are listed below.

Symbolic Name | Undefined
Administrative State | Online
Domain ID | 1
Resource Allocation Timeout (RA TOV) | 10000 milliseconds
Error Detect Timeout (ED TOV) | 2000 milliseconds
IP Address | 10.0.0.1
Subnet Mask Address | 255.0.0.0
Gateway Address | 10.0.0.254.
Network Discovery | RARP
Contact | Undefined
Location | Undefined
Trap Community | Private
Read Community | Public
Write Community | Private
Port State | Online
Port Mode | GL