# SANbox2-64 Menu Bar

The SANbox2-64 menu options displayed depends on whether you are using the topology display or the faceplate display. The topology display menu options are shown below in white background. The faceplate display menu options are shown below in gray background. In addition to the menu bar, both the topology and faceplate displays have context sensitive menus that pop up when you click in the graphic window with the right mouse button.

File Menu

Open View File (Ctrl+O, Alt+F+O) | Opens an existing fabric view file
Save View As (Alt+F+A) | Saves fabric view file to a file
Change Default File Password (Alt+F+D) | Change the Default Fabric View File password
Preferences (Alt+F+P) | Opens the Preferences dialog
Exit (Alt+F+X) | Closes the SANbox Manager application

Fabric Menu

Add a Fabric | Adds a fabric to the topology display
Remove Fabric (Alt+B+R) | Removes a fabric from the topology display
Rediscover Fabric (Alt+B+D) | Clears out the currently displayed fabric information, and rediscovers information on all switches in the fabric
Start Fabric View | Starts the Fabric View application used to monitor port performance
Show Event Browser (Alt+B+E) | Opens the Event Browser in which switch event and alarm information can be filtered and displayed by time-stamp, switch (source), event type, and event description. Can be turned on or off (unavailable) using Preferences dialog.

Switch Menu

Delete (Alt+S+D) | Deletes switch from current fabric view
Export Name Server (Alt+S+E) | Saves name server information to a file
Archive (Alt+S+A) | Saves switch configuration information to a file
Restore (Alt+S+R) | Restores archived switch configuration information to the switch
User Accounts (Alt+S+U) | Opens User Accounts dialog in which to add a new a user, remove a current user, and change the password for a current user.
Set Date/Time (Alt+S+D) | Opens the Switch Date and Time dialog from which to set the date and time on the switch
Hot Swap Wizard (Alt+S+H) | Opens the Hot Swap Wizard consisting of a series of dialogs that walk you through the process of removing, inserting, or replacing an I/O blade
Switch Properties (Alt+S+W) | Opens the Switch Properties dialog
Network Properties (Alt+S+N) | Opens the Network Properties dialog
Toggle Beacon (Alt+S+G) | Sets the LEDs on the switch to blink so you can easily identify the switch
Configure Alarm Thresholds (Alt+S+C) | Opens the Configure Alarm Thresholds dialog in which to set rising/falling thresholds that trigger alarms on the switch
Load Firmware (Alt+S+L) | Opens the Load Firmware dialog from which you can upload and install new firmware to the switch
Activate Firmware (Alt+S+V) | Activates the uploaded firmware.
Firmware Fallback (Alt+S+F) | Opens the Firmware Fallback dialog from which to replace the current firmware image with the other (fallback) firmware image stored on the switch
Reset Switch (Alt+S+E) | Reboots or reinitializes switch to the most recent configuration
Restore Factory Defaults (Alt+S+S) | Restores switch settings to the configuration set at the factory

Blade Menu

Blade Properties (Alt+B+P) | Opens Blade Properties dialog in which to view or change blade properties
Test Blade (Alt+B+T) | Verifies operational status of blade
Reset Blade (Alt+B+E) | Resets blade to the most recent configuration

Port Menu

Port Properties (Alt+P+R) | Opens the Port Properties dialog
Ext Credit Wizard (Alt+P+C) | Opens the Extended Credits Wizard to extend port credits.
Port Symbolic Name (Alt+P+N) | Opens the Port Symbolic Name dialog in which to change the name of a port.
Reset Port (Alt+P+T) | Reinitializes selected port(s)
Port Loopback Test (Alt+P+T) | Runs Internal, External, Online diagnostic test on selected ports

Zoning Menu

Edit Zoning (Alt+Z+E) | Opens the Edit Zoning dialog in which you can change current zone sets
Edit Zoning Config (Alt+Z+C) | Opens the Zoning Config dialog in which to change the FC-SW-2 Auto Save, and Default Visibility settings
Activate Zone Set (Alt+Z+A) | Opens the Activate Zone Set dialog in which to activate a different zone set
Deactivate Zone Set (Alt+Z+D) | Opens the Deactivate Zone Set dialog in which to deactivate the current zone set
Restore Default Zoning (Alt+Z+R) | Restores zoning configuration to the default zoning

View Menu

Refresh (Alt+V+R, F5) | Starts a new polling cycle to update the currently displayed fabric information
Layout Topology | Arrange icons manually
Toggle Auto Layout | SANbox Manager automatically arranges the icons in topology display
Remember Layout | Saves a custom arrangement or layout that can be restored during a later SANbox Manager session
View Port Modes | Displays mode information on port icons in faceplate display
View Port States | Displays state information on port icons in faceplate display
View Port Speeds | Displays speed information on port icons in faceplate display
View Port Media | Displays media information on port icons in faceplate display

Help

Help Topics | Opens the online help file
About… | Displays SANbox Manager software version information