# SANbox Menu Bar

The SANbox with E_Ports menu options displayed depends on whether you are using the topology display or the faceplate display. The topology display menu options are shown below in white background. The faceplate display menu options are shown below in gray background.

File Menu

Open View File | Opens an existing fabric view file
Save View As | Saves fabric view file to the database
Change Default File Password | Change the Default Fabric View File password
Preferences | Opens the Preferences dialog
Exit | Closes the SANbox Manager application

Fabric Menu

Add Fabric | Adds a fabric to the topology display
Remove Fabric | Removes a fabric from the Topology display
Rediscover Fabric | Clears out the currently displayed fabric information, and rediscovers information on all switches in the fabric.

Switch Menu

Delete | Deletes switch from current fabric view
Export Name Server | Saves name server information to a file
Archive | Saves switch configuration information to a file
Restore | Restores archived switch configuration information to the switch
Switch Properties | Opens the Switch Properties dialog
Network Properties | Opens the Network Properties dialog
Toggle Beacon | Sets the LEDs on the switch to blink so you can easily identify the switch
Clear Trap Log | Deletes all trap settings
Export Trap Log | Saves trap log information to a file
Configure Traps | Opens Configure Traps dialog from which you can configure trap conditions
Reset Switch | Reboots or reinitializes switch to the most recent configuration
Restore Factory Defaults | Restores switch settings to the configuration set at the factory

Port Menu

Port Properties | Opens the Port Properties dialog
Extended Credits | Opens the Extended Credits dialog
Port Loopback Test | Runs diagnostic test on an online port connected to a remote device

Zoning Menu

Edit Zoning | Opens the Edit Zoning dialog from which you can change current zone sets
Edit Zoning Config | Opens the Zoning Config dialog in which to change the Default Visibility setting
Activate Zone Set | Opens the Activate Zone Set dialog from which you can activate a different zone set
Deactivate Zone Set | Opens the Deactivate Zone Set dialog from which you can deactivate the current zone set
Restore Default Zoning | Restores zoning configuration to the default zoning

View Menu

Refresh | Starts a new polling cycle to update the currently displayed fabric information
View Port Modes | Displays mode information on port icons in faceplate display
View Port States | Displays state information on port icons in faceplate display
View Port Speeds | Displays speed information on port icons in faceplate display
View Port Media | Displays media information on port icons in faceplate display

Help Menu

Help Topics | Opens the online help file you are now reading
About... | Displays SANbox Manager software version information